# Services

### Designing

We are supported by competent engineers. We provide a service to design a systematic way to produce the best functional product as requested by clients. We apply our scientific knowledge to the solution of technical problems without forgetting on implying the aspect of aesthetical issue.

### Manufacturing, Fabrication

PT Esatama Abadi has the job shop manufacturing process. Each worker is trained to carry out the EHSE system. They all may contribute to the process of making the product. The process of constructing products is by combining typically standardized parts, using one or more individual processes using the range of processes, from the cutting, bending, assembling, etc.

### Installation

-

- All
- Storage Tank
- Pressure Vessel
- Surge Vessel
- Hot Water Tank
- Mixer Tank
- Air Receiver Tank
- Hydrophore Tank

#### Storage Tank

We are involved in manufacturing and supplying storage tanks with a wide variety in shapes and designs. Our storage tanks are available in cone, vertical or horizontal shapes with both closed and open tanks. Theses tanks are useful for containing liquid without pressure system. Features: • Available in various designs and shapes • Capacity from 0,1 up to 100 KL (Small) • Capacity from 20 up to 20.000 KL (Medium) • Capacity above 20.000 KL (Large) • Application: water, fuel, oil, chemical, etc.

#### PRESSURE VESSEL

Our company fabricates Pressure Vessels since long for its valuable clients. The vessels are used for containing pressure with the help of heat supply either from direct source or indirect. They are widely useful for both industrial and private sector applications all over the world. Pressure vessels are very useful in mining, nuclear reactors, oil refineries, submarine, rail and road vehicle airbrake reservoir etc. Features: • Capacity from 0,1 up to 100 KL • Design Pressure up to 100 bar, and even more

#### SURGE VESSEL

Uncontrolled pressure surges in pipelines costs the water industry millions of pounds every year, causing burst pipes, structural damage, negative pressures and colossal water wastage. The surge tank usually consists of a single or double compartment vessel and a level measuring system with sight glasses or magnetic levels. To prevent overpressure and overfilling, the surge tank is fitted with a pressure-relief valve and a high-low level alarm system. Features: • Capacity from 0,1 up to 200 KL • Design Pressure up to 80 bar

#### HOT WATER TANK

Hotels, hospitals and other facilities that need constant supplies of hot water usually have a storage tank that has been sized to meet peak demands, even though the usage at these times exceeds the output of the heater. This is achieved by selecting a tank of sufficient size, with adequate insulation, and designed to prevent incoming cold water from mixing with the hot water supply. Features: • Horizontal or vertical design are available • Capacity from 0,1 up to 100 KL • Design Pressure: ATM up to 40 Bar